;/* 
;  Copyright (c) 2017 Qualcomm Technologies, Inc.
;  All Rights Reserved.
;  Confidential and Proprietary - Qualcomm Technologies, Inc.
;*/

[Version]
Signature          = "$Windows NT$"
Class              = Extension
ClassGUID          = {e2f84ce7-8efa-411c-aa69-97454ca4cb57}
Provider           = %SRFC%
DriverVer = 08/06/2024,1.14.344.0
ExtensionId        = {cf93819f-2a48-4fd9-a076-bfbbe97e6a5d}
CatalogFile.NT     = miscBtExt_x64.cat
PnpLockDown        = 1

[Manufacturer]
%SRFC% = QCABTEXT,NTamd64

; -------------------------------------------------------------------------------------------------------------------------------
; Configure VID/PID(045E/0C9E) to disable LE Audio in x84 platform, and then,  proper BT driver driver will be loaded per VID/PID
; -------------------------------------------------------------------------------------------------------------------------------
[QCABTEXT.NTamd64]
%WCN7851_BT_SWIFT_PAIR_ENABLE_Ext1% = QCABTNVMEXT, USB\VID_045E&PID_0C9E
;%WCN7851_BT_SWIFT_PAIR_ENABLE_Ext1% = QCABTNVMEXT, USB\VID_0CF3&PID_E700



[QCABTNVMEXT]

[QCABTNVMEXT.HW]
AddReg = BTNVMEXT.HW.AddReg

[BTNVMEXT.HW.AddReg]
HKR,,SwiftPairEnabled,0x00010001, 1   ; 1 is defined for swift pair enable. 0 is defined for swift pair disable as default setting.
HKR,,UserNvmFile,0x0000, ramps_0x00190200_1b3b.dfu  ; point driver to correct NVM file

[Strings]
SRFC                                = "Surface"
WCN7851_BT_SWIFT_PAIR_ENABLE_Ext1   = "Qualcomm(R) Bluetooth USB Driver Extension INF"
