; ** COPYRIGHT (C) 2007-2017 Realtek CORPORATION
;
; This product is covered by one or more of the following patents:
; US6,570,884, US6,115,776, and US6,327,625.
;

[Version]
Signature   = "$WINDOWS NT$"
Class       = Multifunction
ClassGuid   = {4d36e971-e325-11ce-bfc1-08002be10318}
Provider    = %Realtek%
DriverVer   = 11/08/2017,1.1.1108.2017
CatalogFile.NT = rtvdevx64.cat

[Manufacturer]
%Realtek% = Realtek, NTamd64

[ControlFlags]
ExcludeFromSelect     = *

[Realtek.NTamd64]
%PTOU% = VDev, PCI\VEN_10EC&DEV_8164
%COM1% = VDev, PCI\VEN_10EC&DEV_816A
%COM2% = VDev, PCI\VEN_10EC&DEV_816B
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C
%BMC%  = VDev, PCI\VEN_10EC&DEV_816E

; 8168DP
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_816A10EC&REV_01
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_816B10EC&REV_01
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_816C10EC&REV_01
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_074C1025&REV_01 ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_074C1025&REV_01 ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_074C1025&REV_01 ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_078A1025&REV_01 ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_078A1025&REV_01 ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_078A1025&REV_01 ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_078B1025&REV_01 ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_078B1025&REV_01 ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_078B1025&REV_01 ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_078D1025&REV_01 ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_078D1025&REV_01 ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_078D1025&REV_01 ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_080A1025&REV_01 ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_080A1025&REV_01 ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_080A1025&REV_01 ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_090C1025&REV_01 ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_090C1025&REV_01 ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_090C1025&REV_01 ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_1002A0A0&REV_01 ;AOPEN
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_1002A0A0&REV_01 ;AOPEN
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_1002A0A0&REV_01 ;AOPEN
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_1005A0A0&REV_01 ;AOPEN
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_1005A0A0&REV_01 ;AOPEN
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_1005A0A0&REV_01 ;AOPEN
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_81681849&REV_01 ;ASROCK
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_81681849&REV_01 ;ASROCK
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_81681849&REV_01 ;ASROCK
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_78301462&REV_01 ;CHANNEL
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_78301462&REV_01 ;CHANNEL
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_78301462&REV_01 ;CHANNEL
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_7ED21019&REV_01 ;ECS
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_7ED21019&REV_01 ;ECS
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_7ED21019&REV_01 ;ECS
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_81DA1019&REV_01 ;ECS
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_81DA1019&REV_01 ;ECS
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_81DA1019&REV_01 ;ECS
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_0DA2105B&REV_01 ;FOXCONN_Clone
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_0DA2105B&REV_01 ;FOXCONN_Clone
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_0DA2105B&REV_01 ;FOXCONN_Clone
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_308817AA&REV_01 ;LENOVO
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_308817AA&REV_01 ;LENOVO
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_308817AA&REV_01 ;LENOVO

; 8168EP
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_816810EC&REV_0E
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_816810EC&REV_0E
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_816810EC&REV_0E
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_08041025&REV_0E ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_08041025&REV_0E ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_08041025&REV_0E ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_10011025&REV_0E ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_10011025&REV_0E ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_10011025&REV_0E ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_10031025&REV_0E ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_10031025&REV_0E ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_10031025&REV_0E ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_10041025&REV_0E ;Acer_vCaptain
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_10041025&REV_0E ;Acer_vCaptain
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_10041025&REV_0E ;Acer_vCaptain
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_10051025&REV_0E ;Acer_vCaptain
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_10051025&REV_0E ;Acer_vCaptain
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_10051025&REV_0E ;Acer_vCaptain
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_100A1025&REV_0E ;Acer_vCaptain
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_100A1025&REV_0E ;Acer_vCaptain
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_100A1025&REV_0E ;Acer_vCaptain
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_100B1025&REV_0E ;Acer_vCaptain
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_100B1025&REV_0E ;Acer_vCaptain
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_100B1025&REV_0E ;Acer_vCaptain
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_101C1025&REV_0E ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_101C1025&REV_0E ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_101C1025&REV_0E ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_10281025&REV_0E ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_10281025&REV_0E ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_10281025&REV_0E ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_10291025&REV_0E ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_10291025&REV_0E ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_10291025&REV_0E ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_10691025&REV_0E ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_10691025&REV_0E ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_10691025&REV_0E ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_106A1025&REV_0E ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_106A1025&REV_0E ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_106A1025&REV_0E ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_10701025&REV_0E ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_10701025&REV_0E ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_10701025&REV_0E ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_10711025&REV_0E ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_10711025&REV_0E ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_10711025&REV_0E ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_10721025&REV_0E ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_10721025&REV_0E ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_10721025&REV_0E ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_11521025&REV_0E ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_11521025&REV_0E ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_11521025&REV_0E ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_11531025&REV_0E ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_11531025&REV_0E ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_11531025&REV_0E ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_11661025&REV_0E ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_11661025&REV_0E ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_11661025&REV_0E ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_11751025&REV_0E ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_11751025&REV_0E ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_11751025&REV_0E ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_11801025&REV_0E ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_11801025&REV_0E ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_11801025&REV_0E ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_119C1025&REV_0E ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_119C1025&REV_0E ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_119C1025&REV_0E ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_12481025&REV_0E ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_12481025&REV_0E ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_12481025&REV_0E ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_124A1025&REV_0E ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_124A1025&REV_0E ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_124A1025&REV_0E ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_124E1025&REV_0E ;Acer
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_124E1025&REV_0E ;Acer
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_124E1025&REV_0E ;Acer
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_81681849&REV_0E ;ASROCK
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_81681849&REV_0E ;ASROCK
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_81681849&REV_0E ;ASROCK
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_85B51043&REV_0E ;ASUS
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_85B51043&REV_0E ;ASUS
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_85B51043&REV_0E ;ASUS
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_81EA1019&REV_0E ;ECS
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_81EA1019&REV_0E ;ECS
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_81EA1019&REV_0E ;ECS
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_81EB1019&REV_0E ;ECS
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_81EB1019&REV_0E ;ECS
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_81EB1019&REV_0E ;ECS
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_9BC61019&REV_0E ;ECS
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_9BC61019&REV_0E ;ECS
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_9BC61019&REV_0E ;ECS
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_9C7F1019&REV_0E ;ECS
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_9C7F1019&REV_0E ;ECS
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_9C7F1019&REV_0E ;ECS
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_0DA7105B&REV_0E ;Foxconn
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_0DA7105B&REV_0E ;Foxconn
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_0DA7105B&REV_0E ;Foxconn
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_0E4C105B&REV_0E ;Foxconn_Clone MB
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_0E4C105B&REV_0E ;Foxconn_Clone MB
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_0E4C105B&REV_0E ;Foxconn_Clone MB
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_12161734&REV_0E ;Fujitsu
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_12161734&REV_0E ;Fujitsu
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_12161734&REV_0E ;Fujitsu
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_E0001458&REV_0E ;Gigabyte
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_E0001458&REV_0E ;Gigabyte
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_E0001458&REV_0E ;Gigabyte
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_221C103C&REV_0E ;HP_Tootsie14/15
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_221C103C&REV_0E ;HP_Tootsie14/15
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_221C103C&REV_0E ;HP_Tootsie14/15
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_221D103C&REV_0E ;HP_Licorice
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_221D103C&REV_0E ;HP_Licorice
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_221D103C&REV_0E ;HP_Licorice
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_8103103C&REV_0E ;HP
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_8103103C&REV_0E ;HP
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_8103103C&REV_0E ;HP
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_83D5103C&REV_0E ;HP
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_83D5103C&REV_0E ;HP
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_83D5103C&REV_0E ;HP
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_83DA103C&REV_0E ;HP
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_83DA103C&REV_0E ;HP
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_83DA103C&REV_0E ;HP
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_83E7103C&REV_0E ;HP
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_83E7103C&REV_0E ;HP
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_83E7103C&REV_0E ;HP
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_83E8103C&REV_0E ;HP
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_83E8103C&REV_0E ;HP
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_83E8103C&REV_0E ;HP
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_83E9103C&REV_0E ;HP
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_83E9103C&REV_0E ;HP
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_83E9103C&REV_0E ;HP
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_8401103C&REV_0E ;HP
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_8401103C&REV_0E ;HP
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_8401103C&REV_0E ;HP
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_8460103C&REV_0E ;HP
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_8460103C&REV_0E ;HP
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_8460103C&REV_0E ;HP
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_8461103C&REV_0E ;HP
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_8461103C&REV_0E ;HP
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_8461103C&REV_0E ;HP
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_8462103C&REV_0E ;HP
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_8462103C&REV_0E ;HP
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_8462103C&REV_0E ;HP
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_8463103C&REV_0E ;HP
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_8463103C&REV_0E ;HP
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_8463103C&REV_0E ;HP
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_8464103C&REV_0E ;HP
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_8464103C&REV_0E ;HP
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_8464103C&REV_0E ;HP
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_30B217AA&REV_0E ;LENOVO
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_30B217AA&REV_0E ;LENOVO
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_30B217AA&REV_0E ;LENOVO
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_30EE17AA&REV_0E ;LENOVO
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_30EE17AA&REV_0E ;LENOVO
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_30EE17AA&REV_0E ;LENOVO
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_30FD17AA&REV_0E ;Lenovo
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_30FD17AA&REV_0E ;Lenovo
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_30FD17AA&REV_0E ;Lenovo
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_310017AA&REV_0E ;Lenovo
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_310017AA&REV_0E ;Lenovo
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_310017AA&REV_0E ;Lenovo
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_310217AA&REV_0E ;Lenovo
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_310217AA&REV_0E ;Lenovo
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_310217AA&REV_0E ;Lenovo
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_311B17AA&REV_0E ;Lenovo
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_311B17AA&REV_0E ;Lenovo
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_311B17AA&REV_0E ;Lenovo
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_313017AA&REV_0E ;Lenovo
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_313017AA&REV_0E ;Lenovo
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_313017AA&REV_0E ;Lenovo
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_36C717AA&REV_0E ;Lenovo
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_36C717AA&REV_0E ;Lenovo
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_36C717AA&REV_0E ;Lenovo
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_504A17AA&REV_0E ;Lenovo
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_504A17AA&REV_0E ;Lenovo
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_504A17AA&REV_0E ;Lenovo
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_511217AA&REV_0E ;Lenovo
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_511217AA&REV_0E ;Lenovo
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_511217AA&REV_0E ;Lenovo
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_511E17AA&REV_0E ;Lenovo
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_511E17AA&REV_0E ;Lenovo
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_511E17AA&REV_0E ;Lenovo
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_79751462&REV_0E ;MSI
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_79751462&REV_0E ;MSI
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_79751462&REV_0E ;MSI
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_01BE1B0A&REV_0E ;PEGATRON
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_01BE1B0A&REV_0E ;PEGATRON
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_01BE1B0A&REV_0E ;PEGATRON
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_01BB1B0A&REV_0E ;Pegatron/SI
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_01BB1B0A&REV_0E ;Pegatron/SI
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_01BB1B0A&REV_0E ;Pegatron/SI
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_01DA1B0A&REV_0E ;Positivo
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_01DA1B0A&REV_0E ;Positivo
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_01DA1B0A&REV_0E ;Positivo

; 8168FP
%PTOU% = VDev, PCI\VEN_10EC&DEV_8164&SUBSYS_816810EC&REV_1A
%COM1% = VDev, PCI\VEN_10EC&DEV_816A&SUBSYS_816810EC&REV_1A
%COM2% = VDev, PCI\VEN_10EC&DEV_816B&SUBSYS_816810EC&REV_1A
%IPMI% = VDev, PCI\VEN_10EC&DEV_816C&SUBSYS_816810EC&REV_1A
%BMC%  = VDev, PCI\VEN_10EC&DEV_816E&SUBSYS_816810EC&REV_1A

[VDev]
Characteristics    = 0x01
Include            = machine.inf
Needs              = NO_DRV

[VDev.Services]
Include            = machine.inf
Needs              = NO_DRV.Services

;------------------------------------------------------------------------------
;  String Definitions
;------------------------------------------------------------------------------

[Strings]
Realtek       = "Realtek"
IPMI          = "Realtek RealManage IPMI"
COM1          = "Realtek RealManage COM1"
COM2          = "Realtek RealManage COM2"
BMC           = "Realtek RealManage BMC"
PTOU          = "Realtek RealManage PTOU"
