;-------------------------------------------------------------------------------
; net7800-x64-n650f.inf
;
; Microchip LAN7800 USB to Ethernet Adapter installation script for x64.
;
; Copyright (c) Microchip Technology Inc.  All rights reserved.

[version]
Signature   = "$Windows NT$"
ClassGUID   = {4d36e972-e325-11ce-bfc1-08002be10318}
Class       = Net
Provider    = %V_MCHP%
DriverPackageDisplayName = %LAN7800.PackageDesc.ntx64%
CatalogFile = atin650f.cat
DriverVer   = 08/10/2018,3.8.4.0

[ControlFlags]


[Manufacturer]
%V_MCHP%=MCHP,ntamd64

[MCHP.ntamd64]

%29M2AF.DeviceDesc%    = 29M2AF_LAN7800.ndi.ntamd64, USB\VID_07C9&PID_0012


;-------------------------------------------------------------------------------
; Microchip LAN7800 USB 3.0 to Ethernet 10/100/1000 Adapter
;
[29M2AF_LAN7800.ndi.ntamd64]
*IfType         = 6                     ; IF_TYPE_ETHERNET_CSMACD 
*MediaType      = 0                     ; NdisMedium802_3
*PhysicalMediaType = 14                 ; NdisPhysicalMedium802_3
Characteristics = 0x84  ; NCF_HAS_UI | NCF_PHYSICAL
BusType         = 15
AddReg          = LAN7800.ndi.reg, LAN7800.params.reg
DelReg          = DelReg.UnusedCaps
CopyFiles       = LAN7800.CopyFiles.ntamd64

[29M2AF_LAN7800.ndi.ntamd64.Services]
AddService      = LAN7800, 2, LAN7800.Service.ntamd64, LAN7800.EventLog.ntamd64

;-----------------------------------------------------------------------------
; Miniport Common
;
[LAN7800.ndi.reg]
HKR,    ,                         BusNumber,           0, "0" 
HKR, Ndi,                         Service,             0, "LAN7800"
HKR, Ndi\Interfaces,              UpperRange,          0, "ndis5"
HKR, Ndi\Interfaces,              LowerRange,          0, "ethernet"

HKLM, SYSTEM\CurrentControlSet\Control\usbflags\042478000100, DisableOnSoftRemove, 1, 01, 00
HKLM, SYSTEM\CurrentControlSet\Control\usbflags\042478050100, DisableOnSoftRemove, 1, 01, 00

[LAN7800.params.reg]

HKR,Ndi\Params\*FlowControl,ParamDesc,      ,%FlowControl%
HKR,Ndi\Params\*FlowControl,type,           ,"enum"
HKR,Ndi\Params\*FlowControl,default,        ,"3"
;;;HKR,Ndi\Params\*FlowControl\enum,"0",       ,%Disabled%
;;;HKR,Ndi\Params\*FlowControl\enum,"1",       ,%Tx_Enabled%
;;;HKR,Ndi\Params\*FlowControl\enum,"2",       ,%Rx_Enabled%
HKR,Ndi\Params\*FlowControl\enum,"3",       ,%Rx_And_Tx_Enabled%

HKR,Ndi\Params\*SpeedDuplex,ParamDesc,      ,%SpeedDuplex%
HKR,Ndi\Params\*SpeedDuplex,type,           ,enum
HKR,Ndi\Params\*SpeedDuplex,default,        ,0
HKR,Ndi\Params\*SpeedDuplex\enum,0,         ,%SpeedDuplex_AutoNeg%


;;;ATI Unused speeds
;;;HKR,Ndi\Params\*SpeedDuplex\enum,1,         ,%SpeedDuplex_10HD%
;;;HKR,Ndi\Params\*SpeedDuplex\enum,2,         ,%SpeedDuplex_10FD%
;;;HKR,Ndi\Params\*SpeedDuplex\enum,3,         ,%SpeedDuplex_100HD%
;;;HKR,Ndi\Params\*SpeedDuplex\enum,4,         ,%SpeedDuplex_100FD%
;;;HKR,Ndi\Params\*SpeedDuplex\enum,6,         ,%SpeedDuplex_1000FD%

HKR,Ndi\Params\AdvertisedCapabilities,ParamDesc,      ,%AdvCapa%
HKR,Ndi\Params\AdvertisedCapabilities,type,           ,enum
HKR,Ndi\Params\AdvertisedCapabilities,default,        ,"10"
;;;HKR,Ndi\Params\AdvertisedCapabilities,optional,       ,1

;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"0",       ,%AdvCapa00%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"1",       ,%AdvCapa01%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"2",       ,%AdvCapa02%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"3",       ,%AdvCapa03%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"4",       ,%AdvCapa04%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"5",       ,%AdvCapa05%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"6",       ,%AdvCapa06%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"7",       ,%AdvCapa07%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"8",       ,%AdvCapa08%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"9",       ,%AdvCapa09%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"A",       ,%AdvCapa10%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"B",       ,%AdvCapa11%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"C",       ,%AdvCapa12%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"D",       ,%AdvCapa13%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"E",       ,%AdvCapa14%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"F",       ,%AdvCapa15%

HKR,Ndi\Params\AdvertisedCapabilities\enum,"10",      ,%AdvCapa16%

;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"11",      ,%AdvCapa17%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"12",      ,%AdvCapa18%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"13",      ,%AdvCapa19%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"14",      ,%AdvCapa20%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"15",      ,%AdvCapa21%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"16",      ,%AdvCapa22%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"17",      ,%AdvCapa23%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"18",      ,%AdvCapa24%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"19",      ,%AdvCapa25%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"1A",      ,%AdvCapa26%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"1B",      ,%AdvCapa27%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"1C",      ,%AdvCapa28%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"1D",      ,%AdvCapa29%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"1E",      ,%AdvCapa30%
;;;HKR,Ndi\Params\AdvertisedCapabilities\enum,"1F",      ,%AdvCapa31%

HKR,Ndi\Params\GigEMasterSlaveMode,ParamDesc,         ,%GigEMasterSlaveMode%
HKR,Ndi\Params\GigEMasterSlaveMode,type,              ,"enum"
HKR,Ndi\Params\GigEMasterSlaveMode,default,           ,"2"
;;;HKR,Ndi\Params\GigEMasterSlaveMode\enum,"0",          ,%GigEForceSlave%
;;;HKR,Ndi\Params\GigEMasterSlaveMode\enum,"1",          ,%GigEForceMaster%
HKR,Ndi\Params\GigEMasterSlaveMode\enum,"2",          ,%GigEAutoMS%

HKR,Ndi\Params\NetworkAddress,ParamDesc,    ,%NetAddr%
HKR,Ndi\Params\NetworkAddress,type,         ,edit
HKR,Ndi\Params\NetworkAddress,LimitText,    ,17
HKR,Ndi\Params\NetworkAddress,UpperCase,    ,1
HKR,Ndi\Params\NetworkAddress,default,      ,""
HKR,Ndi\Params\NetworkAddress,optional,     ,1

HKR,Ndi\Params\*PriorityVLANTag,ParamDesc,  ,%PriorityAndVlan%
HKR,Ndi\Params\*PriorityVLANTag,type,       ,"enum"
HKR,Ndi\Params\*PriorityVLANTag,default,    ,"3"
HKR,Ndi\Params\*PriorityVLANTag\enum,"0",   ,%PVDisabled%
HKR,Ndi\Params\*PriorityVLANTag\enum,"3",   ,%PVEnabled%

HKR,Ndi\Params\VlanID,ParamDesc,            ,%VlanID%
HKR,Ndi\Params\VlanID,type,                 ,"word"
HKR,Ndi\Params\VlanID,default,              ,"0"
HKR,Ndi\Params\VlanID,min,                  ,"0"
HKR,Ndi\Params\VlanID,max,                  ,"4095"
HKR,Ndi\Params\VlanID,step,                 ,"1"
HKR,Ndi\Params\VlanID,base,                 ,"10"

HKR,Ndi\Params\USBBandwidthMode,ParamDesc,  ,%USBBwMode%
HKR,Ndi\Params\USBBandwidthMode,type,       ,"enum"
HKR,Ndi\Params\USBBandwidthMode,default,    ,"0"
HKR,Ndi\Params\USBBandwidthMode\enum,"0",   ,%USBBwMaxTput%
HKR,Ndi\Params\USBBandwidthMode\enum,"1",   ,%USBBwFriendly%
HKR,Ndi\Params\USBBandwidthMode\enum,"2",   ,%USBBwAutomatic%

HKR,Ndi\Params\LTMEnable,ParamDesc,         ,%LTMEnable%
HKR,Ndi\Params\LTMEnable,type,              ,"enum"
HKR,Ndi\Params\LTMEnable,default,           ,"2"
HKR,Ndi\Params\LTMEnable,optional,          ,1
HKR,Ndi\Params\LTMEnable\enum,"2",          ,%HardwareControl%
HKR,Ndi\Params\LTMEnable\enum,"1",          ,%Enabled%
HKR,Ndi\Params\LTMEnable\enum,"0",          ,%Disabled%

HKR,Ndi\Params\LPMEnable,ParamDesc,         ,%LPMEnable%
HKR,Ndi\Params\LPMEnable,type,              ,"enum"
HKR,Ndi\Params\LPMEnable,default,           ,"2"
HKR,Ndi\Params\LPMEnable,optional,          ,1
HKR,Ndi\Params\LPMEnable\enum,"2",          ,%HardwareControl%
HKR,Ndi\Params\LPMEnable\enum,"1",          ,%Enabled%
HKR,Ndi\Params\LPMEnable\enum,"0",          ,%Disabled%

HKR,Ndi\Params\AutoMdix,ParamDesc,          ,%AutoMdix%
HKR,Ndi\Params\AutoMdix,type,               ,"enum"
HKR,Ndi\Params\AutoMdix,default,            ,"2"
HKR,Ndi\Params\AutoMdix\enum,"2",           ,%AMDIXOn%
;;;HKR,Ndi\Params\AutoMdix\enum,"1",           ,%AMDIXOff-Swap%
;;;HKR,Ndi\Params\AutoMdix\enum,"0",           ,%AMDIXOff-Normal%

HKR,Ndi\Params\*WakeOnPattern,ParamDesc,    ,%WakePattern%
HKR,Ndi\Params\*WakeOnPattern,type,         ,enum
HKR,Ndi\Params\*WakeOnPattern,default,      ,1
HKR,Ndi\Params\*WakeOnPattern\enum,0,       ,%WakeDisable%
HKR,Ndi\Params\*WakeOnPattern\enum,1,       ,%WakeEnable%

HKR,Ndi\Params\*WakeOnMagicPacket,ParamDesc,,%WakeMagicPkt%
HKR,Ndi\Params\*WakeOnMagicPacket,type,     ,enum
HKR,Ndi\Params\*WakeOnMagicPacket,default,  ,1
HKR,Ndi\Params\*WakeOnMagicPacket\enum,0,   ,%WakeDisable%
HKR,Ndi\Params\*WakeOnMagicPacket\enum,1,   ,%WakeEnable%

HKR,Ndi\Params\*DeviceSleepOnDisconnect,ParamDesc,    ,%DeviceSleepOnDisconnectDesc%
HKR,Ndi\Params\*DeviceSleepOnDisconnect,type,         ,enum
HKR,Ndi\Params\*DeviceSleepOnDisconnect,default,      ,0
HKR,Ndi\Params\*DeviceSleepOnDisconnect\enum,0,       ,%Disabled%
HKR,Ndi\Params\*DeviceSleepOnDisconnect\enum,1,       ,%Enabled%

HKR,Ndi\Params\*PMARPOffload,ParamDesc,    ,%PMARPOffloadDesc%
HKR,Ndi\Params\*PMARPOffload,type,         ,enum
HKR,Ndi\Params\*PMARPOffload,default,      ,1
HKR,Ndi\Params\*PMARPOffload\enum,0,       ,%Disabled%
HKR,Ndi\Params\*PMARPOffload\enum,1,       ,%Enabled%

HKR,Ndi\Params\*PMNSOffload,ParamDesc,     ,%PMNSOffloadDesc%
HKR,Ndi\Params\*PMNSOffload,type,          ,enum
HKR,Ndi\Params\*PMNSOffload,default,       ,1
HKR,Ndi\Params\*PMNSOffload\enum,0,        ,%Disabled%
HKR,Ndi\Params\*PMNSOffload\enum,1,        ,%Enabled%

HKR,Ndi\Params\*SelectiveSuspend,ParamDesc,         ,%SSuspend%
HKR,Ndi\Params\*SelectiveSuspend,type,              ,enum
HKR,Ndi\Params\*SelectiveSuspend,default,           ,0
HKR,Ndi\Params\*SelectiveSuspend\enum,0,            ,%SSDisable%
HKR,Ndi\Params\*SelectiveSuspend\enum,1,            ,%SSEnable%

HKR,Ndi\Params\*SSIdleTimeout,ParamDesc,    ,%SSIdleTimeout%
HKR,Ndi\Params\*SSIdleTimeout,default,      ,"10"
HKR,Ndi\Params\*SSIdleTimeout,type,         ,"int"
HKR,Ndi\Params\*SSIdleTimeout,min,          ,"1"
HKR,Ndi\Params\*SSIdleTimeout,max,          ,"10"
HKR,Ndi\Params\*SSIdleTimeout,step,         ,"1"
HKR,Ndi\Params\*SSIdleTimeout,base,         ,"10"

HKR,Ndi\Params\*LsoV1IPv4,ParamDesc,    ,%LsoV1IPv4Desc%
HKR,Ndi\Params\*LsoV1IPv4,type,         ,enum
HKR,Ndi\Params\*LsoV1IPv4,default,      ,1
HKR,Ndi\Params\*LsoV1IPv4\enum,0,       ,%Disabled%
HKR,Ndi\Params\*LsoV1IPv4\enum,1,       ,%Enabled%

HKR,Ndi\Params\*LsoV2IPv4,ParamDesc,    ,%LsoV2IPv4Desc%
HKR,Ndi\Params\*LsoV2IPv4,type,         ,enum
HKR,Ndi\Params\*LsoV2IPv4,default,      ,1
HKR,Ndi\Params\*LsoV2IPv4\enum,0,       ,%Disabled%
HKR,Ndi\Params\*LsoV2IPv4\enum,1,       ,%Enabled%

HKR,Ndi\Params\*LsoV2IPv6,ParamDesc,    ,%LsoV2IPv6Desc%
HKR,Ndi\Params\*LsoV2IPv6,type,         ,enum
HKR,Ndi\Params\*LsoV2IPv6,default,      ,1
HKR,Ndi\Params\*LsoV2IPv6\enum,0,       ,%Disabled%
HKR,Ndi\Params\*LsoV2IPv6\enum,1,       ,%Enabled%

HKR,Ndi\Params\*IPChecksumOffloadIPv4,ParamDesc,      ,%IpCsoIPv4%
HKR,Ndi\Params\*IPChecksumOffloadIPv4,type,           ,"enum"
HKR,Ndi\Params\*IPChecksumOffloadIPv4,default,        ,"3"
HKR,Ndi\Params\*IPChecksumOffloadIPv4\enum,"0",       ,%Disabled%
HKR,Ndi\Params\*IPChecksumOffloadIPv4\enum,"1",       ,%TxEnabled%
HKR,Ndi\Params\*IPChecksumOffloadIPv4\enum,"2",       ,%RxEnabled%
HKR,Ndi\Params\*IPChecksumOffloadIPv4\enum,"3",       ,%TxRxEnabled%

HKR,Ndi\Params\*TCPChecksumOffloadIPv4,ParamDesc,      ,%TcpCsoIPv4%
HKR,Ndi\Params\*TCPChecksumOffloadIPv4,type,           ,"enum"
HKR,Ndi\Params\*TCPChecksumOffloadIPv4,default,        ,"3"
HKR,Ndi\Params\*TCPChecksumOffloadIPv4\enum,"0",       ,%Disabled%
HKR,Ndi\Params\*TCPChecksumOffloadIPv4\enum,"1",       ,%TxEnabled%
HKR,Ndi\Params\*TCPChecksumOffloadIPv4\enum,"2",       ,%RxEnabled%
HKR,Ndi\Params\*TCPChecksumOffloadIPv4\enum,"3",       ,%TxRxEnabled%

HKR,Ndi\Params\*TCPChecksumOffloadIPv6,ParamDesc,      ,%TcpCsoIPv6%
HKR,Ndi\Params\*TCPChecksumOffloadIPv6,type,           ,"enum"
HKR,Ndi\Params\*TCPChecksumOffloadIPv6,default,        ,"3"
HKR,Ndi\Params\*TCPChecksumOffloadIPv6\enum,"0",       ,%Disabled%
HKR,Ndi\Params\*TCPChecksumOffloadIPv6\enum,"1",       ,%TxEnabled%
HKR,Ndi\Params\*TCPChecksumOffloadIPv6\enum,"2",       ,%RxEnabled%
HKR,Ndi\Params\*TCPChecksumOffloadIPv6\enum,"3",       ,%TxRxEnabled%

HKR,Ndi\Params\*UDPChecksumOffloadIPv4,ParamDesc,      ,%UdpCsoIPv4%
HKR,Ndi\Params\*UDPChecksumOffloadIPv4,type,           ,"enum"
HKR,Ndi\Params\*UDPChecksumOffloadIPv4,default,        ,"3"
HKR,Ndi\Params\*UDPChecksumOffloadIPv4\enum,"0",       ,%Disabled%
HKR,Ndi\Params\*UDPChecksumOffloadIPv4\enum,"1",       ,%TxEnabled%
HKR,Ndi\Params\*UDPChecksumOffloadIPv4\enum,"2",       ,%RxEnabled%
HKR,Ndi\Params\*UDPChecksumOffloadIPv4\enum,"3",       ,%TxRxEnabled%

HKR,Ndi\Params\*UDPChecksumOffloadIPv6,ParamDesc,      ,%UdpCsoIPv6%
HKR,Ndi\Params\*UDPChecksumOffloadIPv6,type,           ,"enum"
HKR,Ndi\Params\*UDPChecksumOffloadIPv6,default,        ,"3"
HKR,Ndi\Params\*UDPChecksumOffloadIPv6\enum,"0",       ,%Disabled%
HKR,Ndi\Params\*UDPChecksumOffloadIPv6\enum,"1",       ,%TxEnabled%
HKR,Ndi\Params\*UDPChecksumOffloadIPv6\enum,"2",       ,%RxEnabled%
HKR,Ndi\Params\*UDPChecksumOffloadIPv6\enum,"3",       ,%TxRxEnabled%

HKR,Ndi\Params\*JumboPacket,ParamDesc,      ,%JumboMtu%
HKR,Ndi\Params\*JumboPacket,default,        ,"1514"
HKR,Ndi\Params\*JumboPacket,type,           ,"int"
HKR,Ndi\Params\*JumboPacket,min,            ,"1514"
HKR,Ndi\Params\*JumboPacket,max,            ,"9230"
HKR,Ndi\Params\*JumboPacket,step,           ,"1"
HKR,Ndi\Params\*JumboPacket,base,           ,"10"

HKR,Ndi\Params\SleepPhyOnLinkDown,ParamDesc,     ,%EDPD%
HKR,Ndi\Params\SleepPhyOnLinkDown,type,          ,"enum"
HKR,Ndi\Params\SleepPhyOnLinkDown,default,       ,"0"
HKR,Ndi\Params\SleepPhyOnLinkDown\enum,"0",      ,%EDPDOFF%
;;;HKR,Ndi\Params\SleepPhyOnLinkDown\enum,"1",      ,%EDPDON%

HKR,Ndi\Params\*EEE,ParamDesc, ,%EEE%
HKR,Ndi\Params\*EEE,type,      ,enum
HKR,Ndi\Params\*EEE,default,   ,0
HKR,Ndi\Params\*EEE\enum,0,    ,%Disabled%
;;;HKR,Ndi\Params\*EEE\enum,1,    ,%Enabled%

HKR,,DrvCmdMode, 0, "2"

HKR,,MaxBurstBulkIn, 0, "7"
HKR,,MaxBurstBulkOut, 0, "6"

[DelReg.UnusedCaps]
HKR,Ndi\Params\NetDetach
HKR,Ndi\Params\FlowControl
HKR,Ndi\Params\PriorityVLANTag

;-----------------------------------------------------------------------------
; Driver and Service Section
;
[LAN7800.CopyFiles.ntamd64]
atin650f.sys,,,2

[LAN7800.Service.ntamd64]
DisplayName     = %LAN7800.Service.DispName%
ServiceType     = 1 ;%SERVICE_KERNEL_DRIVER%
StartType       = 3 ;%SERVICE_DEMAND_START%
ErrorControl    = 1 ;%SERVICE_ERROR_NORMAL%
ServiceBinary   = %12%\atin650f.sys
LoadOrderGroup  = NDIS

[LAN7800.EventLog.ntamd64]
AddReg = LAN7800.AddEventLog.Reg.ntamd64

[LAN7800.AddEventLog.Reg.ntamd64]
HKR, , EventMessageFile, 0x00020000, "%%SystemRoot%%\System32\netevent.dll;%%SystemRoot%%\System32\Drivers\atin650f.sys"
HKR, , TypesSupported,   0x00010001, 7

;-----------------------------------------------------------------------------
; Files
;
[SourceDisksNames]
1 = %MCHP_DISK_NAME%,,,""

[SourceDisksFiles]
atin650f.sys                       = 1,,

;-----------------------------------------------------------------------------
; DestinationDirs
;
[DestinationDirs]
LAN7800.CopyFiles.ntamd64 = 12

;-----------------------------------------------------------------------------
; Localizable Strings
;
[Strings]
V_MCHP="Microchip Technology Inc."

29M2AF.DeviceDesc          = "Allied Telesis AT-29M2 USB Fiber Ethernet Adapter"


LAN7800.PackageDesc.ntx64   = "LAN78xx USB to Ethernet Adapter x64 Driver"
LAN7800.Service.DispName    = "LAN78xx USB to Ethernet Adapter Service"
MCHP_DISK_NAME="LAN78xx USB to Ethernet Driver Files"

;Parameters and values
FlowControl     = "Flow Control"
Disabled            = "Disabled"
Tx_Enabled          = "Tx Enabled"
Rx_Enabled          = "Rx Enabled"
Rx_And_Tx_Enabled   = "Rx & Tx Advertised"

SpeedDuplex         = "Speed & Duplex"
SpeedDuplex_AutoNeg = "Auto Negotiation"
SpeedDuplex_10HD    = "10 Mbps Half Duplex"
SpeedDuplex_10FD    = "10 Mbps Full Duplex"
SpeedDuplex_100HD   = "100 Mbps Half Duplex"
SpeedDuplex_100FD   = "100 Mbps Full Duplex"
SpeedDuplex_1000FD  = "1.0 Gbps Full Duplex"

AdvCapa		= "Speed Duplex Autonegotiated Advertised Capabilities"
AdvCapa00	= "None"
AdvCapa01	= "10HD"
AdvCapa02	= "10FD"
AdvCapa03	= "10FD & 10HD"
AdvCapa04	= "100HD"
AdvCapa05	= "100HD & 10HD"
AdvCapa06	= "100HD & 10FD"
AdvCapa07	= "100HD, 10FD & 10HD"
AdvCapa08	= "100FD"
AdvCapa09	= "100FD & 10HD"
AdvCapa10	= "100FD & 10FD"
AdvCapa11	= "100FD, 10FD & 10HD"
AdvCapa12	= "100FD & 100HD"
AdvCapa13	= "100FD, 100HD & 10HD"
AdvCapa14	= "100FD, 100HD & 10FD"
AdvCapa15	= "100FD, 100HD, 10FD & 10HD"
AdvCapa16	= "1000FD"
AdvCapa17	= "1000FD & 10HD"
AdvCapa18	= "1000FD & 10FD"
AdvCapa19	= "1000FD, 10FD & 10HD"
AdvCapa20	= "1000FD & 100HD"
AdvCapa21	= "1000FD, 100HD & 10HD"
AdvCapa22	= "1000FD, 100HD & 10FD"
AdvCapa23	= "1000FD, 100HD, 10FD & 10HD"
AdvCapa24	= "1000FD & 100FD"
AdvCapa25	= "1000FD, 100FD & 10HD"
AdvCapa26	= "1000FD, 100FD & 10FD"
AdvCapa27	= "1000FD, 100FD, 10FD & 10HD"
AdvCapa28	= "1000FD, 100FD & 100HD"
AdvCapa29	= "1000FD, 100FD, 100HD & 10HD"
AdvCapa30	= "1000FD, 100FD, 100HD & 10FD"
AdvCapa31	= "All (1000FD, 100FD, 100HD, 10FD & 10HD)"

GigEMasterSlaveMode = "Gigabit Master Slave Mode"
GigEForceSlave      = "Force Slave Mode"
GigEForceMaster     = "Force Master Mode"
GigEAutoMS          = "Auto Detect"

NetAddr         = "Network Address"

PriorityAndVlan = "Packet Priority & VLAN"
PVDisabled      = "Packet Priority & VLAN Disabled"
PVEnabled       = "Packet Priority & VLAN Enabled"
VlanID          = "VLAN ID"

USBBwMode       = "USB Bandwidth Usage Mode"
USBBwMaxTput    = "Maximum Throughput"
USBBwFriendly   = "Sharing Friendly"
USBBwAutomatic  = "Automatic"

HardwareControl = "HW Controlled"

PMARPOffloadDesc = "PM ARP Offload"
PMNSOffloadDesc  = "PM NS Offload"
DeviceSleepOnDisconnectDesc = "Device Sleep On Disconnect"

LsoV1IPv4Desc   = "Large Send Offload V1 (IPv4)"
LsoV2IPv4Desc   = "Large Send Offload V2 (IPv4)"
LsoV2IPv6Desc   = "Large Send Offload V2 (IPv6)"

IpCsoIPv4        = "IPv4 Checksum Offload"
TcpCsoIPv4       = "TCP Checksum Offload (IPv4)"
TcpCsoIPv6       = "TCP Checksum Offload (IPv6)"
UdpCsoIPv4       = "UDP Checksum Offload (IPv4)"
UdpCsoIPv6       = "UDP Checksum Offload (IPv6)"

Enabled         = "Enabled"

TxEnabled       = "Tx Enabled"
RxEnabled       = "Rx Enabled"
TxRxEnabled     = "Rx & Tx Enabled"

JumboMtu        = "Jumbo Frame Size"

NetDetach       = "NetDetach"
NDModeOFF       = "Disabled"
NDModeON        = "Enabled"
NDModeAuto      = "Automatic"

EDPD            = "Power Down Phy on Link Down"
EDPDOFF         = "Disabled"
EDPDON          = "Enabled"

AutoMdix        = "Auto Mdix"
AMDIXOn         = "ON"
AMDIXOff-Swap   = "OFF / Crossed"
AMDIXOff-Normal = "OFF / Straight"

SSuspend        = "Selective Suspend"
SSEnable        = "Enabled"
SSDisable       = "Disabled"

SSIdleTimeout   = "Selective Suspend Idle Timeout"

WakePattern     = "Wake on pattern match"
WakeMagicPkt    = "Wake on magic packet"
WakeDisable     = "Disabled"
WakeEnable      = "Enabled"

LTMEnable       = "USB3 LTM"

LPMEnable       = "USB2 LPM"

EEE             = "Energy-Efficient Ethernet"

[Strings.0011] ; Japanese
V_MCHP="Microchip Technology Inc."

29M2AF.DeviceDesc          = "Allied Telesis AT-29M2 USB Fiber Ethernet Adapter"

LAN7800.PackageDesc.ntx64   = "LAN78xx USB to Ethernet Adapter x64 Driver"
LAN7800.Service.DispName    = "LAN78xx USB to Ethernet Adapter Service"
MCHP_DISK_NAME="LAN78xx USB to Ethernet Driver Files"

;Parameters and values
FlowControl         = "フロー制御"
Disabled            = "無効"
Tx_Enabled          = "送信有効"
Rx_Enabled          = "受信有効"
Rx_And_Tx_Enabled   = "送信/受信有効"

SpeedDuplex         = "速度と半二重/全二重"
SpeedDuplex_AutoNeg = "オートネゴシエーション"
SpeedDuplex_10HD    = "10Mbps/半二重"
SpeedDuplex_10FD    = "10Mbps/全二重"
SpeedDuplex_100HD   = "100Mbps/半二重"
SpeedDuplex_100FD   = "100Mbps/全二重"
SpeedDuplex_1000FD  = "1.0Gbps/全二重"

AdvCapa		= "速度とデュプレックス自動ネゴシエーションアドバタイズ機能"
AdvCapa00	= "None"
AdvCapa01	= "10HD"
AdvCapa02	= "10FD"
AdvCapa03	= "10FD & 10HD"
AdvCapa04	= "100HD"
AdvCapa05	= "100HD & 10HD"
AdvCapa06	= "100HD & 10FD"
AdvCapa07	= "100HD, 10FD & 10HD"
AdvCapa08	= "100FD"
AdvCapa09	= "100FD & 10HD"
AdvCapa10	= "100FD & 10FD"
AdvCapa11	= "100FD, 10FD & 10HD"
AdvCapa12	= "100FD & 100HD"
AdvCapa13	= "100FD, 100HD & 10HD"
AdvCapa14	= "100FD, 100HD & 10FD"
AdvCapa15	= "100FD, 100HD, 10FD & 10HD"
AdvCapa16	= "1000FD"
AdvCapa17	= "1000FD & 10HD"
AdvCapa18	= "1000FD & 10FD"
AdvCapa19	= "1000FD, 10FD & 10HD"
AdvCapa20	= "1000FD & 100HD"
AdvCapa21	= "1000FD, 100HD & 10HD"
AdvCapa22	= "1000FD, 100HD & 10FD"
AdvCapa23	= "1000FD, 100HD, 10FD & 10HD"
AdvCapa24	= "1000FD & 100FD"
AdvCapa25	= "1000FD, 100FD & 10HD"
AdvCapa26	= "1000FD, 100FD & 10FD"
AdvCapa27	= "1000FD, 100FD, 10FD & 10HD"
AdvCapa28	= "1000FD, 100FD & 100HD"
AdvCapa29	= "1000FD, 100FD, 100HD & 10HD"
AdvCapa30	= "1000FD, 100FD, 100HD & 10FD"
AdvCapa31	= "All (1000FD, 100FD, 100HD, 10FD & 10HD)"

GigEMasterSlaveMode = "ギガビットマスタースレーブモード"
GigEForceSlave      = "スレーブモードの強制"
GigEForceMaster     = "マスターモードの強制"
GigEAutoMS          = "自動検出"

NetAddr         = "ネットワークアドレス"

PriorityAndVlan = "優先/VLAN"
PVDisabled      = "優先/VLAN 無効"
PVEnabled       = "優先/VLAN 有効"
VlanID          = "VLAN ID"

USBBwMode       = "USB帯域使用モード"
USBBwMaxTput    = "最大スループット"
USBBwFriendly   = "適切に共有"
USBBwAutomatic  = "自動"

HardwareControl = "ハードウェア制御"

PMARPOffloadDesc = "PM ARP オフロード"
PMNSOffloadDesc  = "PM NS オフロード"
DeviceSleepOnDisconnectDesc = "デバイス スリープ オン ディスコネクト"

LsoV1IPv4Desc   = "大量送信オフロード V1 (IPv4)"
LsoV2IPv4Desc   = "大量送信オフロード V2 (IPv4)"
LsoV2IPv6Desc   = "大量送信オフロード V2 (IPv6)"

IpCsoIPv4        = "IPv4 チェックサム オフロード"
TcpCsoIPv4       = "TCP チェックサム オフロード (IPv4)"
TcpCsoIPv6       = "TCP チェックサム オフロード (IPv6)"
UdpCsoIPv4       = "UDP チェックサム オフロード (IPv4)"
UdpCsoIPv6       = "UDP チェックサム オフロード (IPv6)"

Enabled         = "有効"

TxEnabled       = "送信有効"
RxEnabled       = "受信有効"
TxRxEnabled     = "送信/受信有効"

JumboMtu        = "ジャンボフレームサイズ"

NetDetach       = "ネットデタッチ (NetDetach)"
NDModeOFF       = "無効"
NDModeON        = "有効"
NDModeAuto      = "自動"

EDPD            = "リンクダウン時にPHYをパワーダウンさせる"
EDPDOFF         = "無効"
EDPDON          = "有効"

AutoMdix        = "自動MDIX"
AMDIXOn         = "オン"
AMDIXOff-Swap   = "オフ/クロス"
AMDIXOff-Normal = "オフ/ストレート"

SSuspend        = "セレクティブサスペンド"
SSEnable        = "有効"
SSDisable       = "無効"

SSIdleTimeout   = "セレクティブサスペンド アイドルタイムアウト"

WakePattern     = "ウェイク オン パターンマッチ"
WakeMagicPkt    = "ウェイク オン マジックパケット"
WakeDisable     = "無効"
WakeEnable      = "有効"

LTMEnable       = "USB3 LTM"

LPMEnable       = "USB2 LPM"

EEE             = "省電力イーサネット"